Vermont School Kiln Safety Inspection Checklist
Date of Inspection:
School Name:

Ventilation and Environmental Safety
	Item
	Yes
	No
	N/A
	Corrective Action Needed

	Hazardous kiln fumes and heat are vented directly outdoors.
	☐
	☐
	☐
	

	Kiln ventilation system is functioning properly.
	☐
	☐
	☐
	

	Room has adequate makeup air and general ventilation.
	☐
	☐
	☐
	

	Safety Data Sheets (SDS) are available for all glazing chemicals.
	☐
	☐
	☐
	

	Glazing chemicals are properly stored and disposed of.
	☐
	☐
	☐
	



Housekeeping and Clearance
	Item
	Yes
	No
	N/A
	Corrective Action Needed

	Kiln room is free of combustible materials.
	☐
	☐
	☐
	

	No storage is located near the kiln.
	☐
	☐
	☐
	

	Minimum 18-inch clearance is maintained around the kiln.
	☐
	☐
	☐
	

	Kiln is in a dedicated space or room.
	☐
	☐
	☐
	

	Kiln area can be secured from unauthorized access.
	☐
	☐
	☐
	



Fire Protection
	Item
	Yes
	No
	N/A
	Corrective Action Needed

	Fire extinguisher is located near the kiln.
	☐
	☐
	☐
	

	Fire extinguisher inspection tag is current.
	☐
	☐
	☐
	

	Fire suppression system is installed where required.
	☐
	☐
	☐
	

	High-temperature sprinkler head is installed, if applicable.
	☐
	☐
	☐
	

	Local Fire Marshal has been notified of kiln installation.
	☐
	☐
	☐
	

	Walls have appropriate fire-resistance rating.
	☐
	☐
	☐
	

	No unsealed holes or penetrations exist in walls or ceilings.
	☐
	☐
	☐
	



Equipment Condition
	Item
	Yes
	No
	N/A
	Corrective Action Needed

	Electrical connections show no signs of damage or wear.
	☐
	☐
	☐
	

	Electrical installation appears compliant and professionally installed.
	☐
	☐
	☐
	

	Kiln door closes properly and maintains a seal.
	☐
	☐
	☐
	

	Kiln is free from cracks, structural damage, or deterioration.
	☐
	☐
	☐
	

	Thermostat is functioning properly.
	☐
	☐
	☐
	

	High-limit switch/safety controls are functioning properly.
	☐
	☐
	☐
	

	Manufacturer operating manuals are available.
	☐
	☐
	☐
	




Training and Administrative Controls
	Item
	Yes
	No
	N/A
	Corrective Action Needed

	Kiln operators have received documented safety training.
	☐
	☐
	☐
	

	Staff understand emergency shutdown procedures.
	☐
	☐
	☐
	

	Safety signage is posted and visible.
	☐
	☐
	☐
	

	Warning labels are present and legible.
	☐
	☐
	☐
	

	Emergency contact information is posted.
	☐
	☐
	☐
	

	Inspection and maintenance records are maintained.
	☐
	☐
	☐
	



